365 ALUTEC ROOF OUTLETS

 Manufacturer: Marley Alutec, Unit 1 (G-H), Hudson Road,
 Elms Farm Industrial Estate, Bedford MK41 0LZ
 Tel: 01234 359438, Fax: 01234 357199.
 Email: enquiries@marleyalutec.co.uk
 Reference: Alutec Elite aluminium roof outlet
 Type: Vertical threaded connector – 500mm length
 Product code: AR160

Connection size: 160mm OD

Grate Type: Domed grate

Waterproofing type: Suitable for use with all types (Liquid, single ply, hotmelt, GRP, bituminous etc)

Flow Performance: 19 litres per second

Type / grade: Marine grade Aluminium alloy to BSEN1559:1997,
 BSEN 1676:1997 and BSEN 1706:1998

 Functional life expectancy: 50 years