311 ALIGATOR ALUMINIUM GUTTERS

 Manufacturer: Marley Alutec, Unit 1 (G-H), Hudson Road,
 Elms Farm Industrial Estate, Bedford MK41 0LZ
 Tel: 01234 359438, Fax: 01234 357199.
 Email: enquiries@marleyalutec.co.uk
 Reference: Aligator snap fit Deepflow aluminium rainwater system
 Profile: Deep half round
 Size: 130x80mm

Flow performance: As stated in Alutec literature.
 Outlet Size: 63mmØ, 76mmØ, 102mmØ, 72x72mm, 102x76mm or 102x102mm TBC

 Type / grade: Marine grade extruded aluminium to BS EN 755-2:2008

Finish: Polyester powder coated to BS EN 12206-1:2004

 Colour: TBC
Functional life expectancy: 50 years

Jointing: Internal Snap fit joint union with integral silicone spacers and sealed with Alutec sealant
Fixing: BS EN 1462:2004 Class H, concealed fascia brackets at 750mm centres. Fixed with Alutec austenitic stainless steel 32mm x No. 10 round head screws