365 ALUTEC ROOF OUTLETS  
  
 Manufacturer: Marley Alutec, Unit 1 (G-H), Hudson Road,  
 Elms Farm Industrial Estate, Bedford MK41 0LZ  
 Tel: 01234 359438, Fax: 01234 357199.  
 Email: enquiries@marleyalutec.co.uk  
 Reference: Alutec Elite aluminium balcony outlet   
 Product code: ABO1TG

Connection size: Universal (76mmØ, 72x72mm, 82mmØ or 110mm OD)

Grate Type: Polished stainless steel grate with 300mm adjustable extension ring

Waterproofing type: Suitable for use with all types (Liquid, single ply, hotmelt, GRP, bituminous etc)

Flow Performance: 4.7 litres per second

Type / grade: Marine grade Aluminium alloy to BSEN1559:1997,   
 BSEN 1676:1997 and BSEN 1706:1998

Functional life expectancy: 50 years