365 ALUTEC ROOF OUTLETS  
  
 Manufacturer: Marley Alutec, Unit 1 (G-H), Hudson Road,  
 Elms Farm Industrial Estate, Bedford MK41 0LZ  
 Tel: 01234 359438, Fax: 01234 357199.  
 Email: enquiries@marleyalutec.co.uk  
 Reference: Alutec aluminium roof outlet  
 Type: Balcony outlet  
 Product code: DR360

Connection size: 75mm nominal, 82mm OD

Grate Type: Flat grate

Flow Performance: As stated in Alutec literature.

Type / grade: Marine grade Aluminium alloy to BSEN1559:1997,   
 BSEN 1676:1997 and BSEN 1706:1998

Accessories: Extension ring  
 Functional life expectancy: 50 years