365 ALUTEC ROOF OUTLETS

 Manufacturer: Marley Alutec, Unit 1 (G-H), Hudson Road,
 Elms Farm Industrial Estate, Bedford MK41 0LZ
 Tel: 01234 359438, Fax: 01234 357199.
 Email: enquiries@marleyalutec.co.uk
 Reference: Alutec aluminium roof outlet
 Type: Balcony outlet
 Product code: DR360

Connection size: 75mm nominal, 82mm OD

Grate Type: Flat grate

Flow Performance: As stated in Alutec literature.

 Type / grade: Marine grade Aluminium alloy to BSEN1559:1997,
 BSEN 1676:1997 and BSEN 1706:1998

Accessories: Extension ring
 Functional life expectancy: 50 years